**MATERIAL SAFETY DATA SHEET**

|  |  |
| --- | --- |
| **PRODUCT NAME:** | GreenYard Professional Fertilizer 20-0-5 .37% Prodiamine 20% XCU |

|  |
| --- |
| **SECTION I** |
| MANUFACTURER'S NAME: EMERGENCY TELEPHONE NUMBER CALL |
| GROWMARK FS LLC. DAY OR NIGHT 1-800-424-9300 |
| 3150 STONEY POINT ROAD . TELEPHONE NUMBER FOR INFORMATION: |
| EAST BERLIN PA 17316 (717)-259-9573 (888)-222-4405 |

|  |
| --- |
| **SECTION II CHEMICAL INGREDIENTS / IDENTITY INFORMATION** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CHEMICAL COMPONENTS** | **OSHA PEL** | **ACGIH TLV** | **OTHER**  **LIMITS** | **CAS #** | **%** |
| Urea | 5mg/M3 | 10mg/M3 |  | 57-13-6 |  |
| Iron Sucrate |  |  |  | 1309-37-1 |  |
| Limestone |  |  |  |  |  |
| Clay | 5mg/M3 | 10mg/M3 |  | 1302-78-9 |  |
| Potassium Chloride |  | 10mg/M3 |  | 7447-40-7 |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
| Dithiopyr |  |  |  | 97886-45-8 | .17 |
|  |  |  |  |  |  |

|  |
| --- |
| **SECTION III PHYSICAL / CHEMICAL CHARACTERISTICS** |

|  |  |  |  |
| --- | --- | --- | --- |
| BOILING POINT | NA | SPECIFIC GRAVITY | >1 |
| VAPOR PRESSURE | NA | MELTING POINT | 132.70C |
| VAPOR DENSITY | NA | EVAPORATION RATE | NA |
| SOLUBILITY IN WATER | Soluble | APPEARANCE AND ODOR | Granular & mixed color |

|  |
| --- |
| **SECTION IV FIRE AND EXPLOSION HAZARD DATA** |

|  |
| --- |
| FLASH POINT (METHOD USED): NA |
|  |
| EXTINGUISHING MEDIA: FOAM & WATER |
|  |
| SPECIAL FIRE FIGHTING PROCEDURES: Wear full protective clothing and self-contained breathing apparatus, to protect against the decomposition products of Urea and Sulfur Coated Urea which can be toxic. |
|  |
| UNUSUAL FIRE AND EXPLOSION HAZARDS: Avoid breathing vapors or dust. |

|  |
| --- |
| **SECTION V REACTIVITY DATA** |

|  |  |  |  |
| --- | --- | --- | --- |
| STABLE | X | CONDITIONS TO AVOID | Decomposes when heated above melting point |
| UNSTABLE |  | CONDITIONS TO AVOID |  |

|  |
| --- |
| INCOMPATIBILITY (MATERIALS TO AVOID): Avoid Contact with Strong Acids, |
| Mildly Corrosive to Metals in Presence of Moisture |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| HAZARDOUS DECOMPOSITION OR BY PRODUCTS: NDA | | | | |
|  | | | | |
| HAZARDOUS POLYMERIZATION: | | | |
| MAY OCCUR |  | CONDITIONS TO AVOID |  |
| WILL NOT OCCUR | X | CONDITIONS TO AVOID | N A |

|  |
| --- |
| **SECTION VI HEALTH HAZARD DATA** |
| ROUTES OF ENTRY: Inhalation, Eyes, Skin, and Ingestion |
|  |
| HEALTH HAZARDS: |
| SIGNS AND SYMPTOMS OF EXPOSURE: EYES: Dust and vapors can cause irritation and pain. SKIN: Can cause irritation. INHALATION: Dust can cause sore throat, coughing, and shortness of breath. INGESTION: Can cause sore throat and abdominal pain. |
|  |
| MEDICAL CONDITIONS GENERALLY AGGRAVATED BY EXPOSURE: NDA |
|  |
| EMERGENCY AND FIRST AID PROCEDURES: EYES & INGESTION: Flush immediately with plenty of water, seek medical attention if necessary. SKIN: Remove contaminated clothing immediately and flush contaminated area with water. INHALATION: Move to fresh air and rest. Seek medical attention if necessary. |

|  |
| --- |
| **SECTION VII PRECAUTIONS FOR SAFE HANDLING AND USE** |

|  |
| --- |
| STEPS TO BE TAKEN IN CASE MATERIAL IS RELEASED OR SPILLED: Sweep up and reuse as product. |
|  |
| WASTE DISPOSAL METHOD: Sanitary Landfill. Dispose in compliance with local regulations. |
|  |
| PRECAUTIONS TO BE TAKEN IN HANDLING AND STORING: Store in dry location, remote from acids. |
|  |
| OTHER PRECAUTIONS: |

|  |
| --- |
| **SECTION VIII CONTROL MEASURES / PROCESS AREAS** |

|  |
| --- |
| RESPIRATORY PROTECTION (SPECIFY TYPE): |

|  |  |  |
| --- | --- | --- |
| VENTILATION | LOCAL EXHAUST | as necessary to maintain low dust levels |
|  | MECHANICAL | N A |
|  | SPECIAL | dust mask or respirator in dusty situations |

|  |
| --- |
| PROTECTIVE GLOVES: Gloves recommended EYE PROTECTION: None required |
|  |
| OTHER PROTECTIVE CLOTHING OR EQUIPMENT: Optional |
|  |
| WORK / HYGIENIC PRACTICES: Normally accepted practices. |

|  |
| --- |
| **SECTION IX REGULATORY COMPLIANCE** |

THE FOLLOWING INFORMATION MAY BE USEFUL IN COMPLYING WITH VARIOUS STATE AND FEDERAL LAWS AND REGULATIONS UNDER VARIOUS ENVIRONMENTAL STATUTES:

|  |  |  |  |
| --- | --- | --- | --- |
| REPORTABLE QUANTITY (RQ), EPA REGULATION 40 CFR 302 (CERLA Section 102): | | | |
| **CHEMICAL NAMES** | CAS# | RQ | |
|  |  | NA |

|  |  |  |
| --- | --- | --- |
| THRESHOLD PLANNING QUANTITY (TPQ), EPA REGULATION 40 CFR 355 (SARA Sections 301-304): | | |
| CHEMICAL NAME: | CAS#: | TPQ: |

|  |  |  |  |
| --- | --- | --- | --- |
| TOXIC CHEMICAL RELEASE REPORTING, EPA REGULATION 40 CFR 372 (SARA Section 313): | | | |
| CHEMICAL NAME: | CAS #: | % BY WEIGHT IN PRODUCT |

|  |  |
| --- | --- |
| HAZARDOUS CHEMICAL REPORTING, EPA REGULATION 40 CFR 370 (SARA Sections 311-312): | |
| CHEMICAL NAME: | CAS#: |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| EPA HAZARD CLASSIFICATION CODE: | | | | | |
| ACUTE | CHRONIC | FIRE | PRESSURE | REACTIVE | NOT |
| HAZARD | HAZARD | HAZARD | HAZARD | HAZARD | APPLICABLE |
|  |  |  |  |  | X |

|  |
| --- |
| HAZARD RATING: NFPA |
| \_\_0\_\_FIRE \_\_0\_\_TOXICITY \_\_0\_\_REACTIVITY \_\_U\_\_CORROSIVENESS |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| HAZARD RATING CODE | 0 None | 1 Slight | 2 Moderate | 3 High | U Unknown |

|  |
| --- |
| **SECTION X TRANSPORTATION INFORMATION** |

For further information relative to spills resulting from transportation incidents, refer to latest Department of Transportation Emergency Response Guidebook for Hazardous Material Incidents. DOT P 5800.5

DOT IDENTIFICATION: RQ:

OSHA REQUIRED LABEL INFORMATION:

In compliance with hazard and right-to-know requirements, the following OSHA Hazard Warnings should be found on a label, bill of lading or invoice accompanying this shipment. NA

NOTE: Product label will contain additional non-OSHA related information.

|  |  |  |
| --- | --- | --- |
| DATE: | May 29, 2014 | SUPERSEDES: ALL PREVIOUS |

The information herein was given in good faith but no warranty, expressed or implied was made. Consult for further information.

NA = NOT APPLICABLE NDA = NO DATA AVAILABLE